|  |  |  |  |
| --- | --- | --- | --- |
| ***Requirement #*** | **03** | ***Priority*** | **1** |
| ***Requirement Type*** | **Usability** | ***Use Case*** | **2** |
| ***Description*** | **The luminosity of the lighted digits shall be changeable in brightness during operation. The should range from complete darkness to 10W of outputted light.** | | |
| ***Rationale*** | **The user wants to sleep in a dark and when he wakes up, he wants to read the time.** | | |
| ***Source*** | **User of the alarm clock, clients** | | |
| ***Fit Criterion :*** | **The luminosity levels shall match the levels set by the requirement.** | | |
| ***Supporting material*** |  | ***Annotation1*** |  |

1 Annotation = aantekening  opmerking