|  |  |  |  |
| --- | --- | --- | --- |
| ***Requirement #*** | **06** | ***Priority*** | **1** |
| ***Requirement Type*** | **Functional** | ***Use Case*** | **2** |
| ***Description*** | **The alarm clock should be possible to operate in the following power conditions: 200-240V, 100-120V, 12V & 24V.** | | |
| ***Rationale*** | **The user wants to use the alarm clock at home and on travel.** | | |
| ***Source*** | **User of the alarm clock, clients** | | |
| ***Fit Criterion :*** | **The alarm clock’s operating power shall be within the given conditions.** | | |
| ***Supporting material*** |  | ***Annotation1*** |  |
|  |  |  |  |

1 Annotation = aantekening  opmerking